APPLICATION DETAILS - NEW CONSTRUCTION SECTION VIEWS
STONEDEKS SYSTEM
14600 COMMERCE STREET NE ALLIANCE, OHIO 44601
PHONE: (330) 821-1585
www.stonedeks.com



	
	EXISTING STRUCTURE

	PAVER (OR MANUFACTURED STONE)

	SILCA GRATE
	

	JOISTS
	ATTACHMENT TO EXISTING

	BEAM PER TABLES
	STRUCTURE PER LOCAL
CODE

	UP TO 12" CANTILEVER
	



1'



GRADEGRADELOCALDEPART MENT



JOIST SPAN "L"

6X6 NO.2 SYP TREATED COLUMN, UP TO 10' ABOVE GRADE


CONCRETE FOOTING PADS PER TABLES


DEPTH BUI LDINGBELOWP


DIAMETERTHIC

NEW CONSTRUCTION SECTION
MAXIMUM JOIST SPANS "L" - WHEN USING PAVERS 3/4" TO 3" THICKNESS
	
	NATURAL STONE OR MANUFACTURED CONCRETE PAVER THICKNESS

	JOIST SIZE
	3/4"
	1 1/4"
	2"
	2 1/2"
	3"

	2X6
	8'-9"
	8'-
5"
	7'-10"
	7'-5"
	7'-2"

	2X8
	11'-
4"
	10'-
9"
	10'-0"
	9'-6"
	9'-2"

	2X10
	13'-
7"
	12'-
10"
	11'-
11"
	11'-4"
	10'-
11"

	2X12
	16'-
0"
	15'-
2"
	14'-1"
	13'-4"
	12'-
10"


NOTES:
1. INSTALLATION TO BE COMPLETED IN ACCORDANCE WITH MANUFACTURER'S SPECIFICATIONS.
2. DO NOT SCALE DRAWING.
3. THIS DRAWING IS INTENDED FOR USE BY ARCHITECTS, ENGINEERS, CONTRACTORS, CONSULTANTS AND DESIGN PROFESSIONALS FOR PLANNING PURPOSES ONLY. THIS DRAWING MAY NOT BE USED FOR CONSTRUCTION.
4. FOR PRODUCT AND COMPANY INFORMATION VISIT WWW.STONEDEKS.COM OR CALL
330-821-1585.
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