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[bookmark: Slide 1]Sample construction of Silca System box stairs on any deck platform. Wood boxes are constructed as required to achieve the appropriated riser height and tread width taking into account the height
of the Silca grate (1.5'') and the height of the stone used. The boxes are placed on a Silca grate base to protect against moisture damage.
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For discussion purposes only

[image: ]

[bookmark: Slide 2]Sample construction of Silca Stairs using wood Stair Stringers

Stone steps and fascia
Wood
Stair stringers on 16'' centers










Wood Stair stringers

Silca Grates

Silca grate base for stringers








For discussion purposes only

Cement board can be added to help adhere riser stone
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