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StoneDeks System:  SilcaGrate installation with underdeck drainage systems
There are 2 types of underdeck drainage systems on the market, a trough type that installs on top of the joists with a trough between the joists, and a ceiling type that installs under the joists.  All installations of the underdeck drainage systems should be done according to the local building code and the manufacturer's instructions for the system that you are using.  

The StoneDeks System SilcaGrate™ can then be installed over top of the joists and underdeck drainage system once a self-sealing joist tape is installed on top of the joist, as shown in the diagrams below. 
1.)         Trough style systems: 

Once the trough membrane is installed tape the joints on top of the joists with a self-sealing joist tape and then install the SilcaGrates on top of the joist at the 16” on center joist spacing


[image: image5.png]


 

APPLY TAPE TO THE TOP OF THE TROUGH OVER THE BLOCKING, OR ANYWHERE THERE MAY BE A PENETRATION FROM NAILS OR DECK SCREWS.  TAPE OVER

SEAMS AND ANYWHERE SCREW MAY PENETRATE.
2.) Underdeck drainage / Ceiling Style Systems 
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STEP 5. INSTALLING THE COLLECTOR PANELS

TIP: Installing the Collecior Panelsis easier with wo insialers. With the extured side of he collector panel facing down, sart close
fo the building near the ledger board, and insert one long edge of the collector panel between upper and lower flanges of the Joist
Rails. (see llus. K ). Confinue unilthe firs side is inseried completely. Then, sirfing af the building ner the ledger board, genfly push
up lighty in center of he Collecior Panel unil the ofher long edge slps inf the Joist Rails flanges on the opposie sids of foist space.
Work your way fo ofher end of oist space.
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RUN A WATER TEST


TO ENSURE WATER RUNS TO DOWNSPOUT





TROUGH WILL PITCH 1/4" PER 1' OR MORE








�This membrane is curved downward in the middle and sloped from one end to the other.  You can remove the cup and the "run a water test and add SilcaGrates part way on the top.  If you are able to duplicate this and show 2 or 3 joists in an assembly partially covered with grates that would be good.  Also if you can add a black strip on top of the joist and not it as "self-sealing joist tape."  At the closest end please show a full joist with a downspout underneath it.  


�For this drawing you can close up the collector panel on the left side and then show decking removed, joist tape applied, Silca Grates, and then pavers on top.  
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